**RANAdvisor - Where did the W1314B UMTS HDR control go with 19.0?**

In the 18.x releases and earlier, the UMTS receiver measurement had a property labeled HDR.  Setting it to Yes would slightly reduce the update in exchange for more dynamic range of SC detection. Improvements in measurement speed performance rendered the switch obsolete and it was removed in 19.0